**Dynamic Seismic Analysis of RCC Building as per IS 1893:2002 by Using STAAD-Pro Software**

**Hiteshkumar D. Mishra1, Prof. D.L.Budhlani2**

*1M.Tech-Student Appearing (Structural Engineering)*

*Guru Nanak Institute Of Technology, Dahegaon, Nagpur, India, 441501*

*2Assistant Professor,*

*Guru Nanak Institute Of Technology, Dahegaon, Nagpur, India, 441501*

***Abstract –*** *In this paper seismic response of (G+7)R.C. framed building is analyses for seismic load case by using STAAD-Pro software as per IS1893:2002 part-1.This paper consider different seismic parameter like seismic zone(IV), response reduction factor(R), importance factor(I)& other parameters like rock/soil type, structure type, damping ratio etc. This paper provides complete guidelines for STAAD-Pro software analysis & STAAD –Pro gives the results after run analysis in the STAAD output viewer which shows joint displacements, support reactions, member forces, base shear and lateral load.*

***Keywords-******dynamic analysis, IS 1893:2002, reinforced structure, Earthquake, STAAD-Pro, Seismic loads, multistory building, RCC building.***

**INTRODUCTION**

In general, for design of multistory buildings seismic loads need to be considered. According to IS 1893(Part -1):2002 height of the structure, seismic zone, vertical and horizontal irregularities, soft and weak storey necessitates dynamic analysis for seismic load. Structural engineer’s role becomes challenging when the building is located in a seismic zone. So, it is to design the structure to resist an earthquake. Seismic design stated, as the structure should be able to ensure the minor and frequent shaking intensity without any damage. In Response Spectrum Method, the Time Periods, Natural Frequencies and Mode Shape Coefficients are calculated by STAAD-Pro Software and remaining process will be done by manually. The modal combination rule for Response Spectrum Analysis is SRSS (Square Root Sum of Squares). The main parameters considered in this

Study are seismic zone IV, response reduction factor(R), importance factor (I) and medium soil type.

**METHODOLOGY**

Consider (G+7) storey building located in new Delhi zone IV, the soil conditions is medium stiff soil, entire building is supported on raft foundation, RC frame infill with brick masonry, lumped weight due to dead load is 12kN/m2 on floors and 10kN/m2 on roof, floors carry live load of 4kN/m2 on floors and 1.5kN/m2 on roof, span of building 5m in X and Z direction, Floor to floor height is 3.1m, bottom floor height is 4.2m, size of beam is assume to be as 0.35X0.45m And size of column as 0.35X0.5m, material assume to be concrete. All the supports are assigning as fixed supports,




Fig. 1- fig shows the Structural model of building in STAAD-Pro software.

Calculation of design seismic force by (dynamic) Response spectrum analysis method by using STAAD-PRO software:-

The design lateral shear force is at each floor in each mode is computed by STAAD equation in accordance with equation (7.8.4.5c and7.8.4.5d) from IS 1893-2002.

Where are user inputs

STAAD utilizes the following procedure to generate the lateral seismic load.

1. User provides the value for as factors for input spectrum.
2. Program calculate time periods for first six modes or as specified by the user.
3. Program calculates for each mode utilizing time period and damping ratio for each mode.
4. The program calculates design horizontal acceleration spectrum for different modes.
5. The program then calculates mode participation factor for different modes.
6. The peak lateral seismic force at each floor in each mode is calculated.
7. All response quantities for each mode are calculated.
8. The peak response quantities are then combined as per method (CQC or SRSS or ABS or TEN or CSM) as defined by the user to get the final results.

In order to calculate Base shear value: -

Vb = Ah x W

Seismic parameter:-

1. Seismic zone IV, zone factor Z is 0.24

………… (Table no. 2 of IS1893:2002 Part-1)

1. Response reduction factor, R is 5

………… (Table no. 7 of IS1893:2002 Part-1)

1. Importance factor, I is 1.0

.………... (Table no. 6 of IS1893:2002 Part-1)


Building is made of moment resisting frame with brick in fill panels; we should use empirical expression the fundamental natural period is as follows:


T=0.09h/sqrt (d)……… (Clause 7.6.2 of IS 1893:2002)

Hence approximate fundamental natural period in both X and Z direction is as follows:

T = 0.09(25.9) / sqrt (20)

T = 0.5212 sec… (Since X and Z direction value D = 20)


**Fig. 1- fig shows the seismic parameter**



**Fig. 2- fig shows the seismic load definition**

Floor Loads in Seismic definition


Dead loads and Live loads




**Fig. 3- fig shows the D.L. and L.L.**

**Defining Response Spectrum load Case:-**

First Add Response spectrum load case to load cases. We will have to specify values attach to be considered to calculate the value of Wi.



**Fig. 4- fig shows self weight load in X, Y AND Z-direction**


****

**Fig. 5- fig shows response spectrum load case**


Same way for add self weight load in **Y** and **Z** direction

In Response Spectrum analysis we will have to add floor load (Dead load) in all three direction


**Floor load in X-direction:-**

**Fig. 6- fig shows floor load in X-direction**

**Floor load in Y-Direction:-**


** Fig. 7- fig shows floor load in Y-direction**

**Floor load in Z- direction:-**


****


**Fig. 8- fig shows floor load in Z-direction**

**Roof load in X- direction:-**

**Fig. 9- fig shows roof load in X-direction**


**Roof load in Y- direction:-**

**Fig. 10- fig shows roof load in Y-direction**


**Roof load in Z- direction:-Fig. 11- fig shows roof load in Z-direction**

**Adding Live loads in all directions**


**X- Direction:-**

**Fig. 12- fig shows L.L. in X-direction**

**Y- Direction-**


**Fig. 13- fig shows L.L. in Y-direction**

**Z- Direction-**

****

**Fig. 14- fig shows L.L. in Z-direction**


All this plates will be considered for calculating Wiso to calculate Floor Shear



**Fig. 15- fig shows the load and definition**

Apply Self weight in X, Y and Z to structure


* **Response Spectrum Command**



**Fig. 16- fig shows the response spectrum**

**= = 0.024**


* **Analysis / Print--Mode Shapes**

****

**Fig. 17- fig shows the analyses the mode shapes**

* Click Post Print Command
* Define Commands
* Add-Print Analysis Results
* Add-Storey drift

Analyze the Structure






Fig. 18- fig shows the Joint displacement




Fig. 19- fig shows the Joint displacement




Fig. 20- fig shows the Joint displacement





Fig. 21 fig shows the support reaction

Fig. 22- fig shows the support reaction




Fig. 23- fig shows the member forces




Fig. 24- fig shows the member forces




Fig. 25- fig shows the member forces




Fig. 25- fig shows the base shear

**CONCLUSION**

The response of (G+7) storey RC building under seismic load as per IS1893:2002 (Part-1) by using software STAAD -Pro has been studied. This analysis provides complete guidelines for STAAD-Pro software analysis of dynamic method. STAAD-Pro gives result very quickly as compared to manual calculation. Also Base shear, Lateral load, Joint displacement, support reaction and member forces for all the joints of a building has been calculated in STAAD output viewer.

**REFERENCES**

1. *Bureau of Indian standards: IS 875(Part 1):1987,dead load on 7 structures, new Delhi, india*
2. *Paulay T and Priestley M. J. N, Seismic Design of Reinforced Concrete and Masonry Buildings, Willy Interscience, Canada, 1992*
3. *Li Qiusheng, Cao Hong and Li Guiqing, “Static and Dynamic Analysis of Straight Bars with Variable Cross – Section”, Computers & Structures, Volume: 59, No: 6. Page: 1185 - l 191, 1996.*
4. *Bureau of Indian standards: IS 1893(Part 1):2002indian standard criteria for earthquake resistant design of structure part 1 general provisions of building (fifth revisions), new Delhi india*
5. Bungale S. T, Wind & Earthquake Resistant Buildings Structural Analysis and Design, Monticello, New York 12701, U.S.A, 2005.
6. Agarwal Pankaj, Shrikhande Manish, “Earthquake resistant design of structures”, PHI learning private limited, New Delhi, 2009.
7. BahadornBagheri, Ehsan SaliminFiroozabad, and MohammadrezaYahyaei, “Comparative Study of the Static and Dynamic Analysis of Multi-Storey Irregular Building”, International Journal of Civil, Environmental, and Structural, Construction and Architectural Engineering, Volume: 6, No: 11, 2012.
8. A.K Chopra "Dynamic of structures theory and Earthquake Engineering" fourth edition,Prentice Hall, 2012
9. *P.p.Tapkire, S.J.(2013) Comparative study of highrise building using Indian standards and EURO standards under seismic forces. International journal of science and research(IJSR),1-4.*
10. B. Srikanth, V.Ramesh, “Comparative study of seismic response for seismic coefficient and response spectrum methods” al Int. Journal of Engineering Research and Applications ISSN: 2248-9622, Vol. 3, Issue 5, Sep-Oct2013, pp.1919-1924G.
11. E. Pavan Kumar1, A. Naresh2, M. Nagajyothi3, M. Rajasekhar, “Earthquake Analysis of Multi Storied Residential Building - A Case Study”, 2014.
12. A.K.Chopra , V.S.(2014).Design as per Indian standards and also to determine the effect of providing shear wall to building Mr. Gururaj B. Katti, Dr. Basavraj Balapgol “Seismic Analysis of Multistoried RCC Buildings Due to Mass Irregularity By Time History”, IJERT, Vol: 3(7), pg 2278-0181, 2014
13. Mr. S.Mahesh, M. D. (NOV-DEC 2014). Comparison of analysis and design of regular and irregular configuration of multi Story building in various seismic zones and various types of soils using ETABS and STAAD. IOSR Journal of Mechanical and Civil Engineering (IOSR-JMCE), 1-8.
14. AnirudhGottala, Kintali Sai Nanda Kishore and Dr. Shaik Yajdhani “Comparative Study of Static and Dynamic Seismic Analysis of a Multistoried Building” International Journal of Science Technology & Engineering, Volume 2, Issue 01, July 2015
15. Vinit Dhanvijay , P>D.(2015). Comparative study of different codes in seismic assessment. International research journal of engineering and technology (IRJET),1-13.
16. Mahesh N. Patil, Yogesh N. Sonawane, “Seismic Analysis of Multistoried Building”, International Journal of Engineering and Innovative Technology (IJEIT) Volume 4, Issue 9, March 2015.
17. Chetan Raj, Vivek Verma, Bhupinder Singh, Abhishek ,“Seismic Analysis of Building with Mass and Vertical Geometric Irregularity by Response Spectrum and Seismic Coefficient Method in Zone V and II”, International Journal of Recent Research Aspects ISSN:2349-7688, Vol. 2,Issue 2, June 2015, pp. 204-211.
18. Jun Chen, G.l.(2016). Accelaration response spectrum for predicting f;oor vibration due to occupants jumping.
19. Kumar C.S. (n.d.). Comparision of seismic vulnerability of building designed for Higher force versus Higher ductility.1-13
20. “Comparative Study of the Static and Dynamic Analysis of Multi-Storey Irregular Building” Bahador Bagheri, Ehsan Salimi Firoozabad, and Mohammadreza Yahyaei
21. Document No. :: IITK-GSDMA-EQ21-V2.0 Final Report :: A - Earthquake Codes IITK-GSDMA Project on Building Codes.
22. Staad. Pro Help Menu & Bentley Student Server.

**AUTHOR PROFILE**

|  |  |  |
| --- | --- | --- |
| Sr.No | Photo | Details |
| 1 | E:\HITESHKUMAR\Paper Publish Data\research paper\IMG_20180428_020617.jpg | Hiteshkumar D. Mishra received the B. E. (Civil Engineering) in the year 2015 from MGM’S College of Engineering (SRTMNU Nanded University), Maharashtra State, India. Now he is M.tech. – Student appearing (Structural Engineering) from Gurunanak Institute of Management and Technology, kalmeshwar road, Dahegaon, Nagpur (RTM Nagpur University), Maharashtra State, India. |
| 2 | E:\HITESHKUMAR\Paper Publish Data\research paper\BUDHLANI SIR photo.jpg | Prof.D.L.Budhlani is working as Assistant Professor, department of civil engineering, Guru Nanak institute of Technology, Dahegaon, Nagpur, Maharashtra, India |